package libusb

import "core:c"

// =============================================================================
// Foreign import — platform-selected linking
// =============================================================================

// Set to false to statically link libusb on Windows.
// On Linux/macOS, the system linker decides static vs dynamic based on what's
// available; use pkg-config or linker flags to control it externally.
LIBUSB_SHARED :: #config(LIBUSB_SHARED, true)

//odinfmt: disable
when ODIN_OS == .Windows {
	when ODIN_ARCH == .amd64 {
		when LIBUSB_SHARED {
			foreign import lib "windows-x64/libusb-1.0.lib"
		} else {
			foreign import lib {
				"windows-x64/libusb-1.0-static.lib",
				"system:Advapi32.lib",
				"system:Ole32.lib",
				"system:Setupapi.lib",
			}
		}
	} else when ODIN_ARCH == .i386 {
		when LIBUSB_SHARED {
			foreign import lib "windows-x86/libusb-1.0.lib"
		} else {
			foreign import lib {
				"windows-x86/libusb-1.0-static.lib",
				"system:Advapi32.lib",
				"system:Ole32.lib",
				"system:Setupapi.lib",
			}
		}
	} else {
		#panic("Unsupported Windows architecture for libusb. Only amd64 and i386 are supported.")
	}
} else {
	// Linux, macOS, BSD — link against system-installed libusb.
	// Install via: apt install libusb-1.0-0-dev / brew install libusb / etc.
	foreign import lib "system:usb-1.0"
}
//odinfmt: enable

// libusb API version (1.0.30).
API_VERSION :: 0x0100010C

// Descriptor sizes per descriptor type.
DT_DEVICE_SIZE :: 18
DT_CONFIG_SIZE :: 9
DT_INTERFACE_SIZE :: 9
DT_INTERFACE_ASSOCIATION_SIZE :: 8
DT_ENDPOINT_SIZE :: 7
DT_ENDPOINT_AUDIO_SIZE :: 9
DT_HUB_NONVAR_SIZE :: 7
DT_SS_ENDPOINT_COMPANION_SIZE :: 6
DT_BOS_SIZE :: 5
DT_DEVICE_CAPABILITY_SIZE :: 3

// BOS descriptor sizes.
BT_USB_2_0_EXTENSION_SIZE :: 7
BT_SS_USB_DEVICE_CAPABILITY_SIZE :: 10
BT_SSPLUS_USB_DEVICE_CAPABILITY_SIZE :: 12
BT_CONTAINER_ID_SIZE :: 20
BT_PLATFORM_DESCRIPTOR_MIN_SIZE :: 20

// Maximum BOS descriptor size (sum of all sub-descriptors).
DT_BOS_MAX_SIZE ::
	DT_BOS_SIZE + BT_USB_2_0_EXTENSION_SIZE + BT_SS_USB_DEVICE_CAPABILITY_SIZE + BT_CONTAINER_ID_SIZE

// Endpoint address / direction masks.
ENDPOINT_ADDRESS_MASK :: 0x0f
ENDPOINT_DIR_MASK :: 0x80

// Transfer type mask in bmAttributes.
TRANSFER_TYPE_MASK :: 0x03

// Iso sync type mask in bmAttributes.
ISO_SYNC_TYPE_MASK :: 0x0c

// Iso usage type mask in bmAttributes.
ISO_USAGE_TYPE_MASK :: 0x30

// Control setup packet size (8 bytes).
CONTROL_SETUP_SIZE :: 8

// Total number of error codes in the Error enum.
ERROR_COUNT :: 14

// Hotplug convenience constants.
HOTPLUG_NO_FLAGS :: Hotplug_Flags{}
HOTPLUG_MATCH_ANY :: c.int(-1)

// Maximum length for a device string descriptor in UTF-8 (libusb 1.0.30+).
DEVICE_STRING_BYTES_MAX :: 384

// Poll event constants matching <poll.h> values.
POLLIN :: c.short(0x0001)
POLLPRI :: c.short(0x0002)
POLLOUT :: c.short(0x0004)
POLLERR :: c.short(0x0008)
POLLHUP :: c.short(0x0010)

// Device and/or Interface Class codes.
Class_Code :: enum c.int {
	// In the context of a device descriptor, this bDeviceClass value indicates
	// that each interface specifies its own class information and all interfaces
	// operate independently.
	PER_INTERFACE       = 0x00,
	// Audio class.
	AUDIO               = 0x01,
	// Communications class.
	COMM                = 0x02,
	// Human Interface Device class.
	HID                 = 0x03,
	// Physical.
	PHYSICAL            = 0x05,
	// Image class.
	IMAGE               = 0x06,
	// Printer class.
	PRINTER             = 0x07,
	// Mass storage class.
	MASS_STORAGE        = 0x08,
	// Hub class.
	HUB                 = 0x09,
	// Data class.
	DATA                = 0x0a,
	// Smart Card.
	SMART_CARD          = 0x0b,
	// Content Security.
	CONTENT_SECURITY    = 0x0d,
	// Video.
	VIDEO               = 0x0e,
	// Personal Healthcare.
	PERSONAL_HEALTHCARE = 0x0f,
	// Audio & Video.
	AUDIO_VIDEO         = 0x10,
	// Billboard.
	BILLBOARD           = 0x11,
	// USB Type-C Bridge class.
	TYPE_C_BRIDGE       = 0x12,
	// Bulk Display Protocol.
	BULK_DISPLAY        = 0x13,
	// Management Component Transport Protocol.
	MCTP                = 0x14,
	// I3C class.
	I3C                 = 0x3c,
	// Diagnostic Device.
	DIAGNOSTIC_DEVICE   = 0xdc,
	// Wireless class.
	WIRELESS            = 0xe0,
	// Miscellaneous class.
	MISCELLANEOUS       = 0xef,
	// Application class.
	APPLICATION         = 0xfe,
	// Class is vendor-specific.
	VENDOR_SPEC         = 0xff,
}

// Legacy alias from libusb-0.1.
CLASS_PTP :: Class_Code.IMAGE

// Descriptor types as defined by the USB specification.
Descriptor_Type :: enum c.int {
	// Device descriptor. See `Device_Descriptor`.
	DEVICE                = 0x01,
	// Configuration descriptor. See `Config_Descriptor`.
	CONFIG                = 0x02,
	// String descriptor.
	STRING                = 0x03,
	// Interface descriptor. See `Interface_Descriptor`.
	INTERFACE             = 0x04,
	// Endpoint descriptor. See `Endpoint_Descriptor`.
	ENDPOINT              = 0x05,
	// Interface Association Descriptor. See `Interface_Association_Descriptor`.
	INTERFACE_ASSOCIATION = 0x0b,
	// BOS descriptor.
	BOS                   = 0x0f,
	// Device Capability descriptor.
	DEVICE_CAPABILITY     = 0x10,
	// HID descriptor.
	HID                   = 0x21,
	// HID report descriptor.
	REPORT                = 0x22,
	// Physical descriptor.
	PHYSICAL              = 0x23,
	// Hub descriptor.
	HUB                   = 0x29,
	// SuperSpeed Hub descriptor.
	SUPERSPEED_HUB        = 0x2a,
	// SuperSpeed Endpoint Companion descriptor.
	SS_ENDPOINT_COMPANION = 0x30,
}

// Endpoint direction. Values for bit 7 of the endpoint address.
Endpoint_Direction :: enum c.int {
	// Out: host-to-device.
	OUT = 0x00,
	// In: device-to-host.
	IN  = 0x80,
}

// Endpoint transfer type. Values for bits 0:1 of bmAttributes.
Endpoint_Transfer_Type :: enum c.int {
	// Control endpoint.
	CONTROL     = 0x0,
	// Isochronous endpoint.
	ISOCHRONOUS = 0x1,
	// Bulk endpoint.
	BULK        = 0x2,
	// Interrupt endpoint.
	INTERRUPT   = 0x3,
}

// Standard requests, as defined in table 9-5 of the USB 3.0 specifications.
Standard_Request :: enum c.int {
	// Request status of the specific recipient.
	GET_STATUS        = 0x00,
	// Clear or disable a specific feature.
	CLEAR_FEATURE     = 0x01,
	// Set or enable a specific feature. (0x02 is reserved.)
	SET_FEATURE       = 0x03,
	// Set device address for all future accesses. (0x04 is reserved.)
	SET_ADDRESS       = 0x05,
	// Get the specified descriptor.
	GET_DESCRIPTOR    = 0x06,
	// Used to update existing descriptors or add new descriptors.
	SET_DESCRIPTOR    = 0x07,
	// Get the current device configuration value.
	GET_CONFIGURATION = 0x08,
	// Set device configuration.
	SET_CONFIGURATION = 0x09,
	// Return the selected alternate setting for the specified interface.
	GET_INTERFACE     = 0x0a,
	// Select an alternate interface for the specified interface.
	SET_INTERFACE     = 0x0b,
	// Set then report an endpoint's synchronization frame.
	SYNCH_FRAME       = 0x0c,
	// Sets both the U1 and U2 Exit Latency.
	SET_SEL           = 0x30,
	// Delay from the time a host transmits a packet to the time it is
	// received by the device.
	SET_ISOCH_DELAY   = 0x31,
}

// Request type bits of the bmRequestType field in control transfers.
Request_Type :: enum c.int {
	// Standard.
	STANDARD = 0x00 << 5,
	// Class.
	CLASS    = 0x01 << 5,
	// Vendor.
	VENDOR   = 0x02 << 5,
	// Reserved.
	RESERVED = 0x03 << 5,
}

// Recipient bits of the bmRequestType field in control transfers.
// Values 4 through 31 are reserved.
Request_Recipient :: enum c.int {
	// Device.
	DEVICE    = 0x00,
	// Interface.
	INTERFACE = 0x01,
	// Endpoint.
	ENDPOINT  = 0x02,
	// Other.
	OTHER     = 0x03,
}

// Synchronization type for isochronous endpoints.
// Values for bits 2:3 of bmAttributes.
Iso_Sync_Type :: enum c.int {
	// No synchronization.
	NONE     = 0x0,
	// Asynchronous.
	ASYNC    = 0x1,
	// Adaptive.
	ADAPTIVE = 0x2,
	// Synchronous.
	SYNC     = 0x3,
}

// Usage type for isochronous endpoints.
// Values for bits 4:5 of bmAttributes.
Iso_Usage_Type :: enum c.int {
	// Data endpoint.
	DATA     = 0x0,
	// Feedback endpoint.
	FEEDBACK = 0x1,
	// Implicit feedback data endpoint.
	IMPLICIT = 0x2,
}

// Supported speeds (wSpeedSupported) — bitmask flags.
// Indicates what speeds the device supports.
Supported_Speed_Bit :: enum u16 {
	// Low speed operation supported (1.5MBit/s).
	LOW   = 0,
	// Full speed operation supported (12MBit/s).
	FULL  = 1,
	// High speed operation supported (480MBit/s).
	HIGH  = 2,
	// Superspeed operation supported (5000MBit/s).
	SUPER = 3,
}
Supported_Speeds :: bit_set[Supported_Speed_Bit;u16]

// Masks for the bits of the bmAttributes field of the USB 2.0 Extension
// descriptor.
Usb2_Ext_Attribute_Bit :: enum u32 {
	// Supports Link Power Management (LPM).
	LPM_SUPPORT = 1,
}
Usb2_Ext_Attributes :: bit_set[Usb2_Ext_Attribute_Bit;u32]

// Masks for the bits of the bmAttributes field of the SuperSpeed USB Device
// Capability descriptor.
Ss_Dev_Cap_Attribute_Bit :: enum u8 {
	// Supports Latency Tolerance Messages (LTM).
	LTM_SUPPORT = 1,
}
Ss_Dev_Cap_Attributes :: bit_set[Ss_Dev_Cap_Attribute_Bit;u8]

// USB capability types (BOS).
Bos_Type :: enum c.int {
	// Wireless USB device capability.
	WIRELESS_USB_DEVICE_CAPABILITY = 0x01,
	// USB 2.0 extensions.
	USB_2_0_EXTENSION              = 0x02,
	// SuperSpeed USB device capability.
	SS_USB_DEVICE_CAPABILITY       = 0x03,
	// Container ID type.
	CONTAINER_ID                   = 0x04,
	// Platform descriptor.
	PLATFORM_DESCRIPTOR            = 0x05,
	// SuperSpeedPlus device capability.
	SUPERSPEED_PLUS_CAPABILITY     = 0x0A,
}

// Speed codes. Indicates the speed at which the device is operating.
Speed :: enum c.int {
	// The OS doesn't report or know the device speed.
	UNKNOWN       = 0,
	// The device is operating at low speed (1.5MBit/s).
	LOW           = 1,
	// The device is operating at full speed (12MBit/s).
	FULL          = 2,
	// The device is operating at high speed (480MBit/s).
	HIGH          = 3,
	// The device is operating at super speed (5000MBit/s).
	SUPER         = 4,
	// The device is operating at super speed plus (10000MBit/s).
	SUPER_PLUS    = 5,
	// The device is operating at super speed plus x2 (20000MBit/s).
	SUPER_PLUS_X2 = 6,
}

// Error codes. Most libusb functions return 0 on success or one of these
// codes on failure. Use `error_name()` for a string representation or
// `strerror()` for an end-user description.
Error :: enum c.int {
	// Success (no error).
	SUCCESS       = 0,
	// Input/output error.
	IO            = -1,
	// Invalid parameter.
	INVALID_PARAM = -2,
	// Access denied (insufficient permissions).
	ACCESS        = -3,
	// No such device (it may have been disconnected).
	NO_DEVICE     = -4,
	// Entity not found.
	NOT_FOUND     = -5,
	// Resource busy.
	BUSY          = -6,
	// Operation timed out.
	TIMEOUT       = -7,
	// Overflow.
	OVERFLOW      = -8,
	// Pipe error.
	PIPE          = -9,
	// System call interrupted (perhaps due to signal).
	INTERRUPTED   = -10,
	// Insufficient memory.
	NO_MEM        = -11,
	// Operation not supported or unimplemented on this platform.
	NOT_SUPPORTED = -12,
	// Other error.
	OTHER         = -99,
}

// Transfer type (for the Transfer struct's `type` field).
// Stored as u8 to match libusb_transfer.type which is `unsigned char`.
Transfer_Type :: enum u8 {
	// Control transfer.
	CONTROL     = 0,
	// Isochronous transfer.
	ISOCHRONOUS = 1,
	// Bulk transfer.
	BULK        = 2,
	// Interrupt transfer.
	INTERRUPT   = 3,
	// Bulk stream transfer.
	BULK_STREAM = 4,
}

// Transfer status codes.
Transfer_Status :: enum c.int {
	// Transfer completed without error. Note that this does not indicate that
	// the entire amount of requested data was transferred.
	COMPLETED,
	// Transfer failed.
	ERROR,
	// Transfer timed out.
	TIMED_OUT,
	// Transfer was cancelled.
	CANCELLED,
	// For bulk/interrupt endpoints: halt condition detected (endpoint stalled).
	// For control endpoints: control request not supported.
	STALL,
	// Device was disconnected.
	NO_DEVICE,
	// Device sent more data than requested.
	OVERFLOW,
}

// Transfer flag bits for use in a `Transfer_Flags` bit_set.
Transfer_Flag_Bit :: enum u8 {
	// Report short frames as errors.
	SHORT_NOT_OK,
	// Automatically free() transfer buffer during `free_transfer()`.
	// Do not use with buffers from `dev_mem_alloc()`.
	FREE_BUFFER,
	// Automatically call `free_transfer()` after callback returns.
	// Do not call `free_transfer()` from your callback if this is set.
	FREE_TRANSFER,
	// Terminate transfers that are a multiple of the endpoint's
	// wMaxPacketSize with an extra zero length packet. Currently
	// only supported on Linux. Available since libusb-1.0.9.
	ADD_ZERO_PACKET,
}
Transfer_Flags :: bit_set[Transfer_Flag_Bit;u8]

// Capabilities supported by an instance of libusb on the current running
// platform. Test with `has_capability()`.
Capability :: enum u32 {
	// The `has_capability()` API is available.
	HAS_CAPABILITY                = 0x0000,
	// Hotplug support is available on this platform.
	HAS_HOTPLUG                   = 0x0001,
	// The library can access HID devices without requiring user intervention.
	// Note that before being able to actually access an HID device, you may
	// still have to call additional libusb functions such as
	// `detach_kernel_driver()`.
	HAS_HID_ACCESS                = 0x0100,
	// The library supports detaching of the default USB driver, using
	// `detach_kernel_driver()`, if one is set by the OS kernel.
	SUPPORTS_DETACH_KERNEL_DRIVER = 0x0101,
}

// Log message levels.
Log_Level :: enum c.int {
	// No messages ever emitted by the library (default).
	NONE    = 0,
	// Error messages are emitted.
	ERROR   = 1,
	// Warning and error messages are emitted.
	WARNING = 2,
	// Informational, warning and error messages are emitted.
	INFO    = 3,
	// All messages are emitted.
	DEBUG   = 4,
}

// Log callback mode bits. Since version 1.0.23.
Log_Cb_Mode_Bit :: enum c.int {
	// Callback function handling all log messages.
	GLOBAL  = 0,
	// Callback function handling context related log messages.
	CONTEXT = 1,
}
Log_Cb_Mode :: bit_set[Log_Cb_Mode_Bit;c.int]

// Available option values for `set_option()` and `init_context()`.
Option :: enum c.int {
	// Set the log message verbosity. Argument: `Log_Level` (as c.int).
	//
	// The default level is NONE, which means no messages are ever printed. If
	// you choose to increase the verbosity, ensure your application does not
	// close the stderr file descriptor. Level WARNING is advised.
	//
	// If the LIBUSB_DEBUG environment variable was set when libusb was
	// initialized, this option does nothing. If libusb was compiled without
	// message logging, or with verbose debug logging, this option does nothing.
	LOG_LEVEL           = 0,
	// Use the UsbDk backend for a specific context, if available.
	//
	// This option should be set at initialization with `init_context()`,
	// otherwise unspecified behavior may occur. Only valid on Windows; ignored
	// on all other platforms.
	USE_USBDK           = 1,
	// Do not scan for devices.
	//
	// With this option set, libusb will skip scanning devices in
	// `init_context()`, and hotplug functionality will be deactivated. Useful
	// in combination with `wrap_sys_device()`, which can access a device
	// directly without prior device scanning. This is typically needed on
	// Android, where access to USB devices is limited.
	//
	// Should only be used with `init_context()`, otherwise unspecified behavior
	// may occur. Only valid on Linux; ignored on all other platforms.
	// Alias: WEAK_AUTHORITY.
	NO_DEVICE_DISCOVERY = 2,
	// Set the context log callback function, on a context or globally.
	// Argument: `Log_Cb`. Using this option with a nil context is equivalent
	// to calling `set_log_cb()` with mode GLOBAL; with a non-nil context, it is
	// equivalent to mode CONTEXT.
	LOG_CB              = 3,
	MAX                 = 4,
}

// Alias for NO_DEVICE_DISCOVERY.
OPTION_WEAK_AUTHORITY :: Option.NO_DEVICE_DISCOVERY

// Hotplug event bits. Since version 1.0.16.
Hotplug_Event_Bit :: enum c.int {
	// A device has been plugged in and is ready to use.
	DEVICE_ARRIVED = 0,
	// A device has left and is no longer available. It is the user's
	// responsibility to call `close()` on any associated handle.
	DEVICE_LEFT    = 1,
}
Hotplug_Events :: bit_set[Hotplug_Event_Bit;c.int]

// Hotplug flag bits. Since version 1.0.16.
Hotplug_Flag_Bit :: enum c.int {
	// Arm the callback and fire it for all matching currently attached devices.
	ENUMERATE = 0,
}
Hotplug_Flags :: bit_set[Hotplug_Flag_Bit;c.int]

// Device string type (libusb 1.0.30+).
Device_String_Type :: enum c.int {
	MANUFACTURER,
	PRODUCT,
	SERIAL_NUMBER,
	// The total number of string types.
	COUNT,
}

// Whether a sublink speed attribute defines a symmetric or asymmetric bit
// rate (libusb 1.0.28+).
Ssplus_Sublink_Type :: enum c.int {
	// Symmetric.
	SYM  = 0,
	// Asymmetric.
	ASYM = 1,
}

// Whether a sublink speed attribute defines the receive or transmit bit rate.
Ssplus_Sublink_Direction :: enum c.int {
	// Receive.
	RX = 0,
	// Transmit.
	TX = 1,
}

// Base-10 exponent (times 3) applied to the sublink mantissa.
Ssplus_Sublink_Exponent :: enum c.int {
	// Bits per second.
	BPS = 0,
	// Kbps.
	KBS = 1,
	// Mbps.
	MBS = 2,
	// Gbps.
	GBS = 3,
}

// Protocol supported by a sublink.
Ssplus_Sublink_Protocol :: enum c.int {
	// SuperSpeed.
	SS     = 0,
	// SuperSpeedPlus.
	SSPLUS = 1,
}

// Setup packet for control transfers (8 bytes, packed).
// Use `fill_control_setup()` to populate. The 16-bit fields
// are stored in little-endian byte order on the wire.
Control_Setup :: struct #packed {
	// Request type. Bits 0:4 determine recipient (`Request_Recipient`), bits
	// 5:6 determine type (`Request_Type`), bit 7 determines data transfer
	// direction (`Endpoint_Direction`).
	bmRequestType: u8,
	// Request. If the type bits of bmRequestType are STANDARD then this field
	// refers to `Standard_Request`. Otherwise its use is application-specific.
	bRequest:      u8,
	// Value. Varies according to request.
	wValue:        u16,
	// Index. Varies according to request, typically used to pass an index or
	// offset.
	wIndex:        u16,
	// Number of bytes to transfer.
	wLength:       u16,
}

// Standard USB device descriptor (USB 3.0, section 9.6.1).
// All multi-byte fields in host-endian format.
Device_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:            u8,
	// Descriptor type (`Descriptor_Type.DEVICE`).
	bDescriptorType:    u8,
	// USB spec release number in BCD. 0x0200 = USB 2.0, etc.
	bcdUSB:             u16,
	// USB-IF class code for the device. See `Class_Code`.
	bDeviceClass:       u8,
	// USB-IF subclass code, qualified by bDeviceClass.
	bDeviceSubClass:    u8,
	// USB-IF protocol code, qualified by class and subclass.
	bDeviceProtocol:    u8,
	// Maximum packet size for endpoint 0.
	bMaxPacketSize0:    u8,
	// USB-IF vendor ID.
	idVendor:           u16,
	// USB-IF product ID.
	idProduct:          u16,
	// Device release number in BCD.
	bcdDevice:          u16,
	// Index of manufacturer string descriptor.
	iManufacturer:      u8,
	// Index of product string descriptor.
	iProduct:           u8,
	// Index of serial number string descriptor.
	iSerialNumber:      u8,
	// Number of possible configurations.
	bNumConfigurations: u8,
}

// Standard USB endpoint descriptor (USB 3.0, section 9.6.6).
// All multi-byte fields in host-endian format.
Endpoint_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:          u8,
	// Descriptor type (`Descriptor_Type.ENDPOINT`).
	bDescriptorType:  u8,
	// Endpoint address. Bits 0:3 = endpoint number, bit 7 = direction.
	bEndpointAddress: u8,
	// Endpoint attributes. Bits 0:1 = transfer type, 2:3 = iso sync type,
	// 4:5 = iso usage type.
	bmAttributes:     u8,
	// Maximum packet size this endpoint can send/receive.
	wMaxPacketSize:   u16,
	// Polling interval for data transfers.
	bInterval:        u8,
	// Audio devices only: rate of synchronization feedback.
	bRefresh:         u8,
	// Audio devices only: address of the synch endpoint.
	bSynchAddress:    u8,
	// Extra descriptors. Stored here if libusb encounters unknown descriptors.
	extra:            [^]u8,
	// Length of extra descriptors in bytes.
	extra_length:     c.int,
}

// Standard USB interface association descriptor (USB 3.0, section 9.6.4).
// All multi-byte fields in host-endian format.
Interface_Association_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:           u8,
	// Descriptor type (`Descriptor_Type.INTERFACE_ASSOCIATION`).
	bDescriptorType:   u8,
	// Interface number of the first interface associated with this function.
	bFirstInterface:   u8,
	// Number of contiguous interfaces associated with this function.
	bInterfaceCount:   u8,
	// USB-IF class code for this function. A value of zero is not allowed. If
	// 0xff, the function class is vendor-specific. All other values are
	// reserved for assignment by the USB-IF.
	bFunctionClass:    u8,
	// USB-IF subclass code for this function. If not 0xff, all values are
	// reserved for assignment by the USB-IF.
	bFunctionSubClass: u8,
	// USB-IF protocol code for this function, qualified by bFunctionClass and
	// bFunctionSubClass.
	bFunctionProtocol: u8,
	// Index of string descriptor describing this function.
	iFunction:         u8,
}

// Array of 0 or more interface association descriptors.
Interface_Association_Descriptor_Array :: struct {
	// Array of interface association descriptors. Size determined by `length`.
	iad:    [^]Interface_Association_Descriptor,
	// Number of interface association descriptors contained. Read-only.
	length: c.int,
}

// Standard USB interface descriptor (USB 3.0, section 9.6.5).
// All multi-byte fields in host-endian format.
Interface_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:            u8,
	// Descriptor type (`Descriptor_Type.INTERFACE`).
	bDescriptorType:    u8,
	// Number of this interface.
	bInterfaceNumber:   u8,
	// Value used to select this alternate setting for this interface.
	bAlternateSetting:  u8,
	// Number of endpoints used by this interface (excluding the control
	// endpoint).
	bNumEndpoints:      u8,
	// USB-IF class code for this interface. See `Class_Code`.
	bInterfaceClass:    u8,
	// USB-IF subclass code, qualified by bInterfaceClass.
	bInterfaceSubClass: u8,
	// USB-IF protocol code, qualified by class and subclass.
	bInterfaceProtocol: u8,
	// Index of string descriptor describing this interface.
	iInterface:         u8,
	// Array of endpoint descriptors (length = bNumEndpoints).
	endpoint:           [^]Endpoint_Descriptor,
	// Extra descriptors. Stored here if libusb encounters unknown descriptors.
	extra:              [^]u8,
	// Length of the extra descriptors, in bytes.
	extra_length:       c.int,
}

// A collection of alternate settings for a particular USB interface.
Interface :: struct {
	// Array of interface descriptors (length = num_altsetting).
	altsetting:     [^]Interface_Descriptor,
	// Number of alternate settings that belong to this interface.
	num_altsetting: c.int,
}

// Standard USB configuration descriptor (USB 3.0, section 9.6.3).
// All multi-byte fields in host-endian format.
Config_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:             u8,
	// Descriptor type (`Descriptor_Type.CONFIG`).
	bDescriptorType:     u8,
	// Total length of data returned for this configuration.
	wTotalLength:        u16,
	// Number of interfaces supported by this configuration.
	bNumInterfaces:      u8,
	// Identifier value for this configuration.
	bConfigurationValue: u8,
	// Index of string descriptor describing this configuration.
	iConfiguration:      u8,
	// Configuration characteristics.
	bmAttributes:        u8,
	// Max power consumption. Units of 2 mA (high-speed) or 8 mA (super-speed).
	MaxPower:            u8,
	// Array of interfaces (length = bNumInterfaces).
	interface:           [^]Interface,
	// Extra descriptors. Stored here if libusb encounters unknown descriptors.
	extra:               [^]u8,
	// Length of the extra descriptors, in bytes.
	extra_length:        c.int,
}

// SuperSpeed endpoint companion descriptor (USB 3.0, section 9.6.7).
// All multi-byte fields in host-endian format.
Ss_Endpoint_Companion_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:           u8,
	// Descriptor type (`Descriptor_Type.SS_ENDPOINT_COMPANION`).
	bDescriptorType:   u8,
	// The maximum number of packets the endpoint can send or receive as part
	// of a burst.
	bMaxBurst:         u8,
	// In bulk EP: bits 4:0 represent the maximum number of streams the EP
	// supports. In isochronous EP: bits 1:0 represent the Mult.
	bmAttributes:      u8,
	// The total number of bytes this EP will transfer every service interval.
	// Valid only for periodic EPs.
	wBytesPerInterval: u16,
}

// Generic BOS Device Capability descriptor. Check bDevCapabilityType and
// call the matching get_*_descriptor function for a fully-typed struct.
Bos_Dev_Capability_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:             u8,
	// Descriptor type (`Descriptor_Type.DEVICE_CAPABILITY`).
	bDescriptorType:     u8,
	// Device Capability type. See `Bos_Type`.
	bDevCapabilityType:  u8,
	// Device Capability data (bLength - 3 bytes). Flexible array member.
	dev_capability_data: [0]u8,
}

// Binary Device Object Store (BOS) descriptor (USB 3.0, section 9.6.2).
// All multi-byte fields in host-endian format.
Bos_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:         u8,
	// Descriptor type (`Descriptor_Type.BOS`).
	bDescriptorType: u8,
	// Length of this descriptor and all of its sub descriptors.
	wTotalLength:    u16,
	// The number of separate device capability descriptors in the BOS.
	bNumDeviceCaps:  u8,
	// Flexible array of device capability descriptor pointers.
	dev_capability:  [0]^Bos_Dev_Capability_Descriptor,
}

// USB 2.0 Extension descriptor (USB 3.0, section 9.6.2.1).
// All multi-byte fields in host-endian format.
Usb2_Extension_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:            u8,
	// Descriptor type (`Descriptor_Type.DEVICE_CAPABILITY`).
	bDescriptorType:    u8,
	// Capability type (`Bos_Type.USB_2_0_EXTENSION`).
	bDevCapabilityType: u8,
	// Bitmap of supported device level features. A value of one in a bit
	// location indicates the feature is supported. See `Usb2_Ext_Attributes`.
	bmAttributes:       u32,
}

// SuperSpeed USB Device Capability descriptor (USB 3.0, section 9.6.2.2).
// All multi-byte fields in host-endian format.
Ss_Usb_Device_Capability_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:               u8,
	// Descriptor type (`Descriptor_Type.DEVICE_CAPABILITY`).
	bDescriptorType:       u8,
	// Capability type (`Bos_Type.SS_USB_DEVICE_CAPABILITY`).
	bDevCapabilityType:    u8,
	// Bitmap of supported device level features. A value of one in a bit
	// location indicates the feature is supported. See `Ss_Dev_Cap_Attributes`.
	bmAttributes:          u8,
	// Bitmap of the speeds supported by this device when operating in
	// SuperSpeed mode. See `Supported_Speeds`.
	wSpeedSupported:       u16,
	// The lowest speed at which all the functionality supported by the device
	// is available to the user.
	bFunctionalitySupport: u8,
	// U1 Device Exit Latency.
	bU1DevExitLat:         u8,
	// U2 Device Exit Latency.
	bU2DevExitLat:         u16,
}

// Container ID descriptor (USB 3.0, section 9.6.2.3).
// All multi-byte fields, except UUIDs, in host-endian format.
Container_Id_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:            u8,
	// Descriptor type (`Descriptor_Type.DEVICE_CAPABILITY`).
	bDescriptorType:    u8,
	// Capability type (`Bos_Type.CONTAINER_ID`).
	bDevCapabilityType: u8,
	// Reserved field.
	bReserved:          u8,
	// 128-bit UUID as a byte array.
	ContainerID:        [16]u8,
}

// Platform descriptor (USB 3.2, section 9.6.2.4).
// Contains a flexible array member — all memory must be managed manually.
Platform_Descriptor :: struct {
	// Size of this descriptor (in bytes).
	bLength:                u8,
	// Descriptor type (`Descriptor_Type.DEVICE_CAPABILITY`).
	bDescriptorType:        u8,
	// Capability type (`Bos_Type.PLATFORM_DESCRIPTOR`).
	bDevCapabilityType:     u8,
	// Reserved field.
	bReserved:              u8,
	// 128-bit UUID as a byte array.
	PlatformCapabilityUUID: [16]u8,
	// Capability data (bLength - 20 bytes). Flexible array member.
	CapabilityData:         [0]u8,
}

// SuperSpeedPlus sublink attribute (libusb 1.0.28+, USB 3.1, section 9.6.2.5).
Ssplus_Sublink_Attribute :: struct {
	// Sublink Speed Attribute ID (SSID). Uniquely identifies the speed of this
	// sublink.
	ssid:      u8,
	// Base-10 exponent (times 3) applied to the mantissa.
	exponent:  Ssplus_Sublink_Exponent,
	// Whether the attribute defines a symmetric or asymmetric bit rate.
	type:      Ssplus_Sublink_Type,
	// Whether the attribute defines the receive or transmit bit rate.
	direction: Ssplus_Sublink_Direction,
	// The protocol supported by the link.
	protocol:  Ssplus_Sublink_Protocol,
	// Mantissa applied to the exponent when calculating the maximum bit rate.
	mantissa:  u16,
}

// SuperSpeedPlus USB Device Capability descriptor (libusb 1.0.28+).
// This is a parsed/computed representation, not the raw USB descriptor.
Ssplus_Usb_Device_Capability_Descriptor :: struct {
	// Sublink Speed Attribute Count.
	numSublinkSpeedAttributes: u8,
	// Sublink Speed ID Count.
	numSublinkSpeedIDs:        u8,
	// Unique ID to indicate the minimum lane speed.
	ssid:                      u8,
	// Minimum receive lane count.
	minRxLaneCount:            u8,
	// Minimum transmit lane count.
	minTxLaneCount:            u8,
	// Flexible array of sublink attributes (length = numSublinkSpeedAttributes).
	sublinkSpeedAttributes:    [0]Ssplus_Sublink_Attribute,
}

// Version of the libusb runtime.
Version :: struct {
	// Library major version.
	major:    u16,
	// Library minor version.
	minor:    u16,
	// Library micro version.
	micro:    u16,
	// Library nano version. Deprecated since 1.0.31: this value is frozen and
	// no longer updated per build. Use `describe` for a unique-per-build
	// identifier.
	nano:     u16,
	// Library release candidate suffix string, e.g. "-rc4".
	rc:       cstring,
	// Human-readable build identifier (never nil). Intended for display, logs,
	// and bug reports; the overall format is not stable, do not parse.
	describe: cstring,
}

// Isochronous packet descriptor.
Iso_Packet_Descriptor :: struct {
	// Length of data to request in this packet.
	length:        c.uint,
	// Amount of data that was actually transferred.
	actual_length: c.uint,
	// Status code for this packet.
	status:        Transfer_Status,
}

// Generic USB transfer structure.
Transfer :: struct {
	// Handle of the device that this transfer will be submitted to.
	dev_handle:      Device_Handle,
	// Bitwise OR of `Transfer_Flags`.
	flags:           Transfer_Flags,
	// Address of the endpoint where this transfer will be sent.
	endpoint:        u8,
	// Type of the transfer from `Transfer_Type`.
	type:            Transfer_Type,
	// Timeout for this transfer in milliseconds. 0 = no timeout.
	timeout:         c.uint,
	// Status of the transfer. Read-only, valid only within the callback.
	status:          Transfer_Status,
	// Length of the data buffer.
	length:          c.int,
	// Actual length of data transferred. Read-only, valid only within callback.
	actual_length:   c.int,
	// Callback invoked when the transfer completes, fails, or is cancelled.
	callback:        Transfer_Cb,
	// User context data accessible from within the callback.
	user_data:       rawptr,
	// Data buffer.
	buffer:          [^]u8,
	// Number of isochronous packets. Only for isochronous endpoints.
	num_iso_packets: c.int,
	// Isochronous packet descriptors. Flexible array member.
	iso_packet_desc: [0]Iso_Packet_Descriptor,
}

// Platform-specific timeval struct matching the system's struct timeval.
// libusb uses this for event-loop timeouts.
when ODIN_OS == .Darwin {
	Timeval :: struct {
		tv_sec:  c.long,
		tv_usec: i32,
	}
} else {
	Timeval :: struct {
		tv_sec:  c.long,
		tv_usec: c.long,
	}
}

// File descriptor for polling.
Poll_Fd :: struct {
	fd:     c.int,
	// Event flags from <poll.h>. POLLIN for read-ready, POLLOUT for write-ready.
	events: c.short,
}

// Option value union for `Init_Option`.
Init_Option_Value :: struct #raw_union {
	// An integer value used by the option (if applicable).
	ival:   c.int,
	// A log callback value used by the option (if applicable).
	log_cb: Log_Cb,
}

// Option structure for `init_context()`.
Init_Option :: struct {
	// Which option to set.
	option: Option,
	// The value to set the option to (if the option takes one).
	value:  Init_Option_Value,
}

//----- Opaque handles ----------------------------------

Context :: distinct rawptr
Device :: distinct rawptr
Device_Handle :: distinct rawptr

// Hotplug callback handle, returned by `hotplug_register_callback()`.
Callback_Handle :: distinct c.int

//----- Callback types ----------------------------------

// Asynchronous transfer callback. When submitting asynchronous transfers, you
// pass a pointer to a callback of this type via the `callback` member of the
// `Transfer`. libusb calls this later, when the transfer has completed or
// failed.
Transfer_Cb :: #type proc "c" (transfer: ^Transfer)

// Callback function for handling log messages. `ctx` is the context related to
// the message, or nil for a global message. `level` is the log level and `str`
// is the message. Since version 1.0.23.
Log_Cb :: #type proc "c" (ctx: Context, level: Log_Level, str: cstring)

// Hotplug event callback. When requesting hotplug notifications, you pass a
// pointer to a callback of this type. It may be called by an internal event
// thread, so it is recommended to do minimal processing before returning. It
// is safe to call `hotplug_register_callback()` or
// `hotplug_deregister_callback()` from within the callback. Return true to
// indicate this callback is finished processing events (deregistering it).
// Since version 1.0.16.
Hotplug_Callback_Fn :: #type proc "c" (
	ctx: Context,
	device: Device,
	event: Hotplug_Events,
	user_data: rawptr,
) -> b32

// Callback invoked when a new file descriptor should be added to the set of
// file descriptors monitored for events.
Pollfd_Added_Cb :: #type proc "c" (fd: c.int, events: c.short, user_data: rawptr)

// Callback invoked when a file descriptor should be removed from the set being
// monitored for events. After returning, do not use that file descriptor again.
Pollfd_Removed_Cb :: #type proc "c" (fd: c.int, user_data: rawptr)

@(default_calling_convention = "c", link_prefix = "libusb_")
foreign lib {

	// ---- Library initialization/deinitialization ----

	// Set the log handler. libusb redirects its log messages to `cb`. Per-context
	// and global messages are supported; context messages also go to the global
	// handler. `ctx` may be nil for the default context (ignored when only the
	// GLOBAL mode is requested). Pass a nil `cb` to stop redirection.
	// Since version 1.0.23.
	set_log_cb :: proc(ctx: Context, cb: Log_Cb, mode: Log_Cb_Mode) ---
	// Set an option in the library. Some options require arguments; consult each
	// `Option`. If `ctx` is nil, the option is added to a list of defaults
	// applied to all subsequently created contexts. Returns SUCCESS, or
	// INVALID_PARAM / NOT_SUPPORTED / NOT_FOUND. Since version 1.0.22.
	set_option :: proc(ctx: Context, option: Option, #c_vararg args: ..any) -> Error ---
	// Deprecated initialization function, equivalent to `init_context(ctx, nil, 0)`.
	// Must be called before any other libusb function. If `ctx` is nil, a default
	// context is created (or reused).
	init :: proc(ctx: ^Context) -> Error ---
	// Initialize libusb. Must be called before any other libusb function. If you
	// do not provide an output location for a context pointer, a default context
	// is created (and reused if one already exists). If `num_options` is 0 then
	// `options` is ignored and may be nil. Returns SUCCESS or an Error.
	// Since version 1.0.27.
	init_context :: proc(ctx: ^Context, options: [^]Init_Option, num_options: c.int) -> Error ---
	// Deinitialize libusb. Should be called after closing all open devices and
	// before your application terminates. `ctx` may be nil for the default context.
	exit :: proc(ctx: Context) ---

	// Deprecated: use `set_option(.LOG_LEVEL, level)` instead.
	set_debug :: proc(ctx: Context, level: c.int) ---

	// ---- Device handling and enumeration ----

	// Returns a list of USB devices currently attached to the system. You must
	// later free the list with `free_device_list()` (which can optionally unref
	// the devices). Be careful not to unref a device you are about to open until
	// after you have opened it. Returns the number of devices in the list (the
	// list is NULL-terminated, so it is actually one element larger), or a
	// negative Error code.
	get_device_list :: proc(ctx: Context, list: ^[^]Device) -> int ---
	// Free a list of devices obtained from `get_device_list()`. If `unref_devices`
	// is true, the reference count of each device in the list is decremented by 1.
	free_device_list :: proc(list: [^]Device, unref_devices: b32) ---
	// Get the number of the bus that a device is connected to.
	get_bus_number :: proc(dev: Device) -> u8 ---
	// Get the number of the port that a device is connected to. Usually uniquely
	// tied to a physical port. Returns 0 if not available.
	get_port_number :: proc(dev: Device) -> u8 ---
	// Get the list of all port numbers from root for the specified device.
	// `port_numbers_len` is the max length of the array (max depth is 7 per the
	// USB 3.0 spec). Returns the number of elements filled, or OVERFLOW if the
	// array is too small. Since version 1.0.16.
	get_port_numbers :: proc(dev: Device, port_numbers: [^]u8, port_numbers_len: c.int) -> c.int ---
	// Deprecated: use `get_port_numbers()` instead.
	get_port_path :: proc(ctx: Context, dev: Device, path: [^]u8, path_length: u8) -> c.int ---
	// Get the parent of the specified device. Returns the parent, or nil if not
	// available. Only valid between a `get_device_list()` / `free_device_list()`
	// pair.
	get_parent :: proc(dev: Device) -> Device ---
	// Get the address of the device on the bus it is connected to.
	get_device_address :: proc(dev: Device) -> u8 ---
	// Get the negotiated connection speed for a device. Returns a `Speed` code;
	// UNKNOWN means the OS doesn't know or doesn't support reporting it.
	get_device_speed :: proc(dev: Device) -> Speed ---
	// Returns the backend-specific identifier of the underlying system device
	// tree node. Since version 1.0.30.
	get_session_data :: proc(dev: Device) -> c.ulong ---
	// Convenience function to retrieve the wMaxPacketSize value for an endpoint
	// in the active device configuration. Returns the wMaxPacketSize value, or
	// NOT_FOUND / OTHER. For iso transfers prefer `get_max_iso_packet_size()`.
	get_max_packet_size :: proc(dev: Device, endpoint: u8) -> c.int ---
	// Calculate the maximum packet size an endpoint is capable of sending or
	// receiving in 1 microframe. Useful when setting up isochronous transfers.
	// Returns the max packet size, or NOT_FOUND / OTHER.
	get_max_iso_packet_size :: proc(dev: Device, endpoint: u8) -> c.int ---
	// Like `get_max_iso_packet_size()` but for a specific interface and alternate
	// setting rather than the first one. Since version 1.0.27.
	get_max_alt_packet_size :: proc(dev: Device, interface_number: c.int, alternate_setting: c.int, endpoint: u8) -> c.int ---
	// Increment the reference count of a device. Returns the same device.
	ref_device :: proc(dev: Device) -> Device ---
	// Decrement the reference count of a device. The device is destroyed when its
	// reference count reaches 0.
	unref_device :: proc(dev: Device) ---
	// Wrap a platform-specific system device handle to obtain a libusb device
	// handle. On Linux, `sys_dev` must be a valid file descriptor opened on the
	// device node. The system handle must remain open until `close()` and is not
	// closed by `close()`. Since version 1.0.23.
	wrap_sys_device :: proc(ctx: Context, sys_dev: c.intptr_t, dev_handle: ^Device_Handle) -> Error ---
	// Open a device and obtain a device handle, which allows you to perform I/O.
	// Adds a reference to the device (removed by `close()`). Returns SUCCESS, or
	// NO_MEM / ACCESS / NO_DEVICE.
	open :: proc(dev: Device, dev_handle: ^Device_Handle) -> Error ---
	// Convenience function to open the first device with the given vendor/product
	// IDs. Not intended for real applications (e.g. it only returns the first
	// match). Returns a device handle, or nil on error / if not found.
	open_device_with_vid_pid :: proc(ctx: Context, vendor_id: u16, product_id: u16) -> Device_Handle ---
	// Close a device handle. Should be called on all open handles before your
	// application exits. Destroys the reference added by `open()`.
	close :: proc(dev_handle: Device_Handle) ---
	// Get the underlying device for a device handle. Does not modify the device's
	// reference count, so you need not unref the result.
	get_device :: proc(dev_handle: Device_Handle) -> Device ---
	// Determine the bConfigurationValue of the currently active configuration.
	// May use OS caches (no I/O) or block on a control transfer. Writes 0 to
	// `config` if the device is unconfigured. Returns SUCCESS or NO_DEVICE.
	get_configuration :: proc(dev_handle: Device_Handle, config: ^c.int) -> Error ---
	// Set the active configuration for a device. A value of -1 puts the device in
	// an unconfigured state. Calling with the already-active value acts as a
	// lightweight reset. Cannot change configuration while interfaces are claimed.
	// Blocking. Returns SUCCESS, or NOT_FOUND / BUSY / NOT_SUPPORTED / NO_DEVICE.
	set_configuration :: proc(dev_handle: Device_Handle, configuration: c.int) -> Error ---
	// Claim an interface on a device handle. Must be claimed before performing
	// I/O on any of its endpoints. Purely logical (no bus I/O). Returns SUCCESS,
	// or NOT_FOUND / BUSY / NO_DEVICE.
	claim_interface :: proc(dev_handle: Device_Handle, interface_number: c.int) -> Error ---
	// Release a previously claimed interface. Release all claimed interfaces
	// before closing a handle. Blocking (sends a SET_INTERFACE request). Returns
	// SUCCESS, or NOT_FOUND / NO_DEVICE.
	release_interface :: proc(dev_handle: Device_Handle, interface_number: c.int) -> Error ---
	// Activate an alternate setting for an interface (which must be claimed).
	// Blocking. Returns SUCCESS, or NOT_FOUND / NO_DEVICE.
	set_interface_alt_setting :: proc(dev_handle: Device_Handle, interface_number: c.int, alternate_setting: c.int) -> Error ---
	// Clear the halt/stall condition for an endpoint. Cancel all pending
	// transfers on the endpoint first. Blocking. Returns SUCCESS, or NOT_FOUND /
	// NO_DEVICE.
	clear_halt :: proc(dev_handle: Device_Handle, endpoint: u8) -> Error ---
	// Perform a USB port reset to reinitialize a device. If the reset fails or
	// the descriptors change, returns NOT_FOUND — close the handle and
	// re-enumerate. Blocking, usually with a noticeable delay.
	reset_device :: proc(dev_handle: Device_Handle) -> Error ---
	// Determine if a kernel driver is active on an interface. If active, you
	// cannot claim the interface. Not available on Windows. Returns 0 if no
	// kernel driver is active, 1 if active, or a negative Error code.
	kernel_driver_active :: proc(dev_handle: Device_Handle, interface_number: c.int) -> c.int ---
	// Detach a kernel driver from an interface, allowing you to claim it. Not
	// available on Windows. Returns SUCCESS, or NOT_FOUND / INVALID_PARAM /
	// NO_DEVICE / NOT_SUPPORTED.
	detach_kernel_driver :: proc(dev_handle: Device_Handle, interface_number: c.int) -> Error ---
	// Re-attach an interface's kernel driver previously detached with
	// `detach_kernel_driver()`. Not available on Windows. Returns SUCCESS, or
	// NOT_FOUND / INVALID_PARAM / NO_DEVICE / NOT_SUPPORTED / BUSY.
	attach_kernel_driver :: proc(dev_handle: Device_Handle, interface_number: c.int) -> Error ---
	// Enable/disable libusb's automatic kernel driver detachment. When enabled,
	// libusb detaches the kernel driver on `claim_interface()` and re-attaches it
	// on `release_interface()`. Returns SUCCESS, or NOT_SUPPORTED on platforms
	// without this capability.
	set_auto_detach_kernel_driver :: proc(dev_handle: Device_Handle, enable: b32) -> Error ---

	// ---- Miscellaneous ----

	// Check at runtime if the loaded library has a given capability. Should be
	// performed after `init_context()`, so the backend has updated its capability
	// set. Returns nonzero if the capability is supported, 0 otherwise.
	has_capability :: proc(capability: Capability) -> c.int ---
	// Returns a constant string with the ASCII name of an Error or transfer
	// status code (e.g. "LIBUSB_ERROR_IO"). Must not be freed.
	error_name :: proc(errcode: Error) -> cstring ---
	// Returns a pointer to a `Version` with the version of the running library.
	get_version :: proc() -> ^Version ---
	// Set the language used for translatable libusb messages (see `strerror()`).
	// `locale` is a 2-letter ISO 639-1 code, optionally followed by region.
	// Returns SUCCESS, or INVALID_PARAM / NOT_FOUND. Since version 1.0.21.
	setlocale :: proc(locale: cstring) -> Error ---
	// Returns a constant UTF-8 string describing an Error code, suitable for
	// display to an end user. Must not be freed.
	strerror :: proc(errcode: Error) -> cstring ---

	// ---- USB descriptors ----

	// Get the USB device descriptor for a device. Non-blocking; the descriptor is
	// cached. Returns SUCCESS or an Error.
	get_device_descriptor :: proc(dev: Device, desc: ^Device_Descriptor) -> Error ---
	// Get the configuration descriptor for the currently active configuration.
	// Free with `free_config_descriptor()`. Returns SUCCESS, or NOT_FOUND if the
	// device is in an unconfigured state.
	get_active_config_descriptor :: proc(dev: Device, config: ^^Config_Descriptor) -> Error ---
	// Get a configuration descriptor by its index. Free with
	// `free_config_descriptor()`. Returns SUCCESS, or NOT_FOUND.
	get_config_descriptor :: proc(dev: Device, config_index: u8, config: ^^Config_Descriptor) -> Error ---
	// Get a configuration descriptor with a specific bConfigurationValue. Free
	// with `free_config_descriptor()`. Returns SUCCESS, or NOT_FOUND.
	get_config_descriptor_by_value :: proc(dev: Device, bConfigurationValue: u8, config: ^^Config_Descriptor) -> Error ---
	// Free a configuration descriptor obtained from `get_active_config_descriptor()`
	// or `get_config_descriptor()`. Safe to call with nil.
	free_config_descriptor :: proc(config: ^Config_Descriptor) ---
	// Get the SuperSpeed endpoint companion descriptor for an endpoint. Free with
	// `free_ss_endpoint_companion_descriptor()`. Returns SUCCESS, NOT_FOUND if not
	// present, or another Error.
	get_ss_endpoint_companion_descriptor :: proc(ctx: Context, endpoint: ^Endpoint_Descriptor, ep_comp: ^^Ss_Endpoint_Companion_Descriptor) -> Error ---
	// Free an SS endpoint companion descriptor. Safe to call with nil.
	free_ss_endpoint_companion_descriptor :: proc(ep_comp: ^Ss_Endpoint_Companion_Descriptor) ---
	// Get a Binary Object Store (BOS) descriptor. Free with `free_bos_descriptor()`.
	// Returns SUCCESS, NOT_FOUND if not present, or another Error.
	get_bos_descriptor :: proc(dev_handle: Device_Handle, bos: ^^Bos_Descriptor) -> Error ---
	// Free a BOS descriptor. Safe to call with nil.
	free_bos_descriptor :: proc(bos: ^Bos_Descriptor) ---
	// Get a USB 2.0 Extension descriptor from a BOS device capability. Free with
	// `free_usb2_extension_descriptor()`. Returns SUCCESS or an Error.
	get_usb2_extension_descriptor :: proc(ctx: Context, dev_cap: ^Bos_Dev_Capability_Descriptor, usb2_extension: ^^Usb2_Extension_Descriptor) -> Error ---
	// Free a USB 2.0 Extension descriptor. Safe to call with nil.
	free_usb2_extension_descriptor :: proc(usb2_extension: ^Usb2_Extension_Descriptor) ---
	// Get a SuperSpeed USB Device Capability descriptor from a BOS device
	// capability. Free with `free_ss_usb_device_capability_descriptor()`. Returns
	// SUCCESS or an Error.
	get_ss_usb_device_capability_descriptor :: proc(ctx: Context, dev_cap: ^Bos_Dev_Capability_Descriptor, ss_usb_device_cap: ^^Ss_Usb_Device_Capability_Descriptor) -> Error ---
	// Free a SuperSpeed USB Device Capability descriptor. Safe to call with nil.
	free_ss_usb_device_capability_descriptor :: proc(ss_usb_device_cap: ^Ss_Usb_Device_Capability_Descriptor) ---
	// Get a SuperSpeedPlus USB Device Capability descriptor from a BOS device
	// capability. Free with `free_ssplus_usb_device_capability_descriptor()`.
	// Since version 1.0.27.
	get_ssplus_usb_device_capability_descriptor :: proc(ctx: Context, dev_cap: ^Bos_Dev_Capability_Descriptor, ssplus_usb_device_cap: ^^Ssplus_Usb_Device_Capability_Descriptor) -> Error ---
	// Free a SuperSpeedPlus USB Device Capability descriptor. Safe to call with
	// nil. Since version 1.0.27.
	free_ssplus_usb_device_capability_descriptor :: proc(ssplus_usb_device_cap: ^Ssplus_Usb_Device_Capability_Descriptor) ---
	// Get a Container ID descriptor from a BOS device capability. Free with
	// `free_container_id_descriptor()`. Returns SUCCESS or an Error.
	get_container_id_descriptor :: proc(ctx: Context, dev_cap: ^Bos_Dev_Capability_Descriptor, container_id: ^^Container_Id_Descriptor) -> Error ---
	// Free a Container ID descriptor. Safe to call with nil.
	free_container_id_descriptor :: proc(container_id: ^Container_Id_Descriptor) ---
	// Get a Platform descriptor from a BOS device capability. Free with
	// `free_platform_descriptor()`. Since version 1.0.27.
	get_platform_descriptor :: proc(ctx: Context, dev_cap: ^Bos_Dev_Capability_Descriptor, platform_descriptor: ^^Platform_Descriptor) -> Error ---
	// Free a Platform descriptor. Safe to call with nil. Since version 1.0.27.
	free_platform_descriptor :: proc(platform_descriptor: ^Platform_Descriptor) ---
	// Retrieve a string descriptor in C-style ASCII. `data` is an output buffer
	// of size `length`. Returns the number of bytes written, or a negative Error
	// code.
	get_string_descriptor_ascii :: proc(dev_handle: Device_Handle, desc_index: u8, data: [^]u8, length: c.int) -> c.int ---
	// Get an array of interface association descriptors (IADs) for a given
	// configuration index. Free with `free_interface_association_descriptors()`.
	// Since version 1.0.27.
	get_interface_association_descriptors :: proc(dev: Device, config_index: u8, iad_array: ^^Interface_Association_Descriptor_Array) -> Error ---
	// Get an array of IADs for the currently active configuration. Free with
	// `free_interface_association_descriptors()`. Since version 1.0.27.
	get_active_interface_association_descriptors :: proc(dev: Device, iad_array: ^^Interface_Association_Descriptor_Array) -> Error ---
	// Free an array of interface association descriptors. Safe to call with nil.
	// Since version 1.0.27.
	free_interface_association_descriptors :: proc(iad_array: ^Interface_Association_Descriptor_Array) ---

	// ---- Device string (libusb 1.0.30+) ----

	// Retrieve a device string descriptor (manufacturer, product, or serial
	// number) as UTF-8. `data` is an output buffer of size `length`. Returns the
	// number of bytes written (including the null terminator), or a negative
	// Error code. Since version 1.0.30.
	get_device_string :: proc(dev: Device, string_type: Device_String_Type, data: [^]u8, length: c.int) -> c.int ---

	// ---- Raw I/O (libusb 1.0.30+) ----

	// Check whether an endpoint supports WinUSB RAW_IO. Only endpoints using the
	// WinUSB driver support it; all other backends return 0. The interface must
	// be claimed. Returns 1 if supported, 0 if not, or a negative Error code.
	// Since version 1.0.30.
	endpoint_supports_raw_io :: proc(dev_handle: Device_Handle, endpoint: u8) -> c.int ---
	// Enable/disable WinUSB RAW_IO for an endpoint on an open device. Can greatly
	// improve throughput. While enabled, transfers must obey alignment rules: the
	// buffer length must be a multiple of the endpoint's max packet size and
	// `<= get_max_raw_io_transfer_size()`. Returns 0 (SUCCESS), or a negative
	// Error code (NOT_SUPPORTED if the backend lacks RAW_IO). Since version 1.0.30.
	endpoint_set_raw_io :: proc(dev_handle: Device_Handle, endpoint: u8, enable: b32) -> c.int ---
	// Retrieve the maximum transfer size in bytes supported for WinUSB RAW_IO on
	// an inbound bulk or interrupt endpoint. Returns a positive maximum transfer
	// size, or a negative Error code (NOT_SUPPORTED if unsupported). Since version
	// 1.0.30.
	get_max_raw_io_transfer_size :: proc(dev_handle: Device_Handle, endpoint: u8) -> c.int ---

	// ---- Device hotplug event notification ----

	// Register a hotplug callback. It fires when a matching event occurs on a
	// matching device, until deregistered or until the callback returns true.
	// Pass `HOTPLUG_MATCH_ANY` for vendor_id / product_id / dev_class to match
	// anything. If `flags` includes ENUMERATE, the callback also fires for all
	// currently attached matching devices. `callback_handle` may be nil. Returns
	// SUCCESS or an Error. Since version 1.0.16.
	hotplug_register_callback :: proc(ctx: Context, events: Hotplug_Events, flags: Hotplug_Flags, vendor_id: c.int, product_id: c.int, dev_class: c.int, cb_fn: Hotplug_Callback_Fn, user_data: rawptr, callback_handle: ^Callback_Handle) -> Error ---
	// Deregister a hotplug callback. Safe to call from within a hotplug callback.
	// Since version 1.0.16.
	hotplug_deregister_callback :: proc(ctx: Context, callback_handle: Callback_Handle) ---
	// Get the user_data associated with a hotplug callback. Since version 1.0.24.
	hotplug_get_user_data :: proc(ctx: Context, callback_handle: Callback_Handle) -> rawptr ---

	// ---- Asynchronous device I/O ----

	// Allocate up to `num_streams` USB bulk streams on the specified endpoints
	// (which must all belong to the same interface). Stream id 0 is reserved; if
	// N streams are allocated you may use ids 1..=N. Returns the number of streams
	// allocated, or a negative Error code. Since version 1.0.19.
	alloc_streams :: proc(dev_handle: Device_Handle, num_streams: u32, endpoints: [^]u8, num_endpoints: c.int) -> c.int ---
	// Free bulk streams allocated with `alloc_streams()`. Streams are also freed
	// automatically when releasing an interface. Returns SUCCESS or an Error.
	// Since version 1.0.19.
	free_streams :: proc(dev_handle: Device_Handle, endpoints: [^]u8, num_endpoints: c.int) -> Error ---
	// Attempt to allocate a block of persistent DMA memory suitable for transfers
	// against the device, allowing zero-copy. Returns nil on failure (many systems
	// do not support this). Free with `dev_mem_free()`; do not use the FREE_BUFFER
	// flag on such buffers. Since version 1.0.21.
	dev_mem_alloc :: proc(dev_handle: Device_Handle, length: c.size_t) -> [^]u8 ---
	// Free device memory allocated with `dev_mem_alloc()`. Returns SUCCESS or an
	// Error.
	dev_mem_free :: proc(dev_handle: Device_Handle, buffer: [^]u8, length: c.size_t) -> Error ---
	// Allocate a transfer with the given number of isochronous packet descriptors
	// (0 for control/bulk/interrupt). The returned transfer is pre-initialized.
	// Free with `free_transfer()`. Returns nil on error.
	alloc_transfer :: proc(iso_packets: c.int) -> ^Transfer ---
	// Free a transfer allocated with `alloc_transfer()`. If the FREE_BUFFER flag
	// is set and the buffer is non-nil, the buffer is also freed. Safe to call
	// with nil. It is illegal to free an active (submitted, incomplete) transfer.
	free_transfer :: proc(transfer: ^Transfer) ---
	// Submit a transfer. Fires off the transfer and returns immediately. Returns
	// SUCCESS, or NO_DEVICE / BUSY / NOT_SUPPORTED / INVALID_PARAM / another Error.
	submit_transfer :: proc(transfer: ^Transfer) -> Error ---
	// Asynchronously cancel a previously submitted transfer. Returns immediately;
	// the callback is invoked later with status CANCELLED. Returns SUCCESS, or
	// NOT_FOUND if the transfer is not in progress / already complete / already
	// cancelled.
	cancel_transfer :: proc(transfer: ^Transfer) -> Error ---
	// Set a transfer's bulk stream id. Prefer `fill_bulk_stream_transfer()`.
	// Since version 1.0.19.
	transfer_set_stream_id :: proc(transfer: ^Transfer, stream_id: u32) ---
	// Get a transfer's bulk stream id. Since version 1.0.19.
	transfer_get_stream_id :: proc(transfer: ^Transfer) -> u32 ---

	// ---- Polling and timing ----

	// Attempt to acquire the event handling lock, which ensures only one thread
	// monitors libusb's event sources at a time. Only needed if you poll()/select()
	// on libusb's file descriptors directly. Returns 0 if the lock was obtained,
	// 1 if it was not.
	try_lock_events :: proc(ctx: Context) -> c.int ---
	// Acquire the event handling lock, blocking until it is obtained. Only needed
	// if you poll()/select() on libusb's file descriptors directly.
	lock_events :: proc(ctx: Context) ---
	// Release the lock acquired with `try_lock_events()` or `lock_events()`. Wakes
	// up any threads blocked on `wait_for_event()`.
	unlock_events :: proc(ctx: Context) ---
	// Determine if it is still OK for this thread to be doing event handling. Call
	// before polling; if it returns false, give up the events lock and retry the
	// cycle. Returns true if event handling can start or continue, false if this
	// thread must give up the events lock.
	event_handling_ok :: proc(ctx: Context) -> b32 ---
	// Determine if an active thread is handling events (i.e. holds the event
	// handling lock). Returns true if a thread is handling events, false if none.
	event_handler_active :: proc(ctx: Context) -> b32 ---
	// Interrupt any active thread that is handling events. Mainly useful for
	// interrupting a dedicated event-handling thread before calling `exit()`.
	// Since version 1.0.21.
	interrupt_event_handler :: proc(ctx: Context) ---
	// Acquire the event waiters lock. Use when you want to be notified of event
	// completion but another thread is handling events.
	lock_event_waiters :: proc(ctx: Context) ---
	// Release the event waiters lock.
	unlock_event_waiters :: proc(ctx: Context) ---
	// Wait for another thread to signal completion of an event. Must be called
	// with the event waiters lock held. Blocks until the timeout expires, a
	// transfer completes, or a thread releases the event handling lock. `tv` may
	// be nil for an unlimited wait. Returns 0 after a transfer completes or
	// another thread stops handling events, 1 if the timeout expired, or
	// INVALID_PARAM.
	wait_for_event :: proc(ctx: Context, tv: ^Timeval) -> c.int ---
	// Handle any pending events in blocking mode (60s internal timeout). Kept
	// mainly for backwards compatibility; prefer `handle_events_completed()`.
	// Returns SUCCESS or an Error.
	handle_events :: proc(ctx: Context) -> Error ---
	// Handle any pending events, blocking up to `tv` (an all-zero timeval gives
	// non-blocking behavior). Kept for backwards compatibility; prefer
	// `handle_events_timeout_completed()`. Returns SUCCESS or an Error.
	handle_events_timeout :: proc(ctx: Context, tv: ^Timeval) -> Error ---
	// Like `handle_events_timeout()`, but if `completed` is non-nil this returns
	// immediately (after obtaining the event lock) once the pointed-to flag is
	// set, allowing race-free waiting for a specific transfer. The flag should be
	// set from within the transfer callback. Returns SUCCESS, or INVALID_PARAM /
	// another Error.
	handle_events_timeout_completed :: proc(ctx: Context, tv: ^Timeval, completed: ^b32) -> Error ---
	// Like `handle_events()`, with a `completed` flag for race-free waiting on a
	// specific transfer (see `handle_events_timeout_completed()`). Returns SUCCESS
	// or an Error.
	handle_events_completed :: proc(ctx: Context, completed: ^b32) -> Error ---
	// Handle pending events by polling file descriptors, without checking whether
	// other threads are already doing so. Must be called with the event lock held.
	// Returns SUCCESS, or INVALID_PARAM / another Error.
	handle_events_locked :: proc(ctx: Context, tv: ^Timeval) -> Error ---
	// Determine whether your application must apply special timing considerations
	// when monitoring libusb's file descriptors. Returns 0 if you must call into
	// libusb at times determined by `get_next_timeout()`, or 1 if all timeout
	// events are handled internally or through regular file-descriptor activity.
	pollfds_handle_timeouts :: proc(ctx: Context) -> c.int ---
	// Determine the next internal timeout that libusb needs to handle. Only needed
	// if you poll()/select() on libusb's file descriptors yourself; use the result
	// as an upper bound for your poll timeout. Returns 0 if there are no pending
	// timeouts, 1 if a timeout was returned, or a negative Error code.
	get_next_timeout :: proc(ctx: Context, tv: ^Timeval) -> c.int ---
	// Register notification functions for file-descriptor additions/removals as
	// libusb's event sources change. Pass nil function pointers to remove the
	// notifiers. Note that descriptors may already have been added before you
	// register (e.g. at `init_context()` time).
	set_pollfd_notifiers :: proc(ctx: Context, added_cb: Pollfd_Added_Cb, removed_cb: Pollfd_Removed_Cb, user_data: rawptr) ---
	// Retrieve the list of file descriptors that should be polled as libusb event
	// sources. Returns a NULL-terminated list of `Poll_Fd` pointers; free with
	// `free_pollfds()`. Not available on Windows (returns nil).
	get_pollfds :: proc(ctx: Context) -> [^]^Poll_Fd ---
	// Free a pollfd list obtained from `get_pollfds()`. Safe to call with nil.
	// Since version 1.0.20.
	free_pollfds :: proc(pollfds: [^]^Poll_Fd) ---

	// ---- Synchronous device I/O ----

	// Perform a USB control transfer. `data` must point to a buffer of `wLength`
	// bytes for the data stage (direction per bit 7 of `bmRequestType`). `timeout`
	// is in milliseconds (0 = unlimited). Returns the number of bytes actually
	// transferred, or a negative Error code.
	control_transfer :: proc(dev_handle: Device_Handle, bmRequestType: u8, bRequest: u8, wValue: u16, wIndex: u16, data: [^]u8, wLength: u16, timeout: c.uint) -> c.int ---
	// Perform a USB bulk transfer. `transferred`, if non-nil, receives the number
	// of bytes actually transferred. `timeout` is in milliseconds (0 = unlimited).
	// Returns SUCCESS, or TIMEOUT / PIPE / OVERFLOW / NO_DEVICE / another Error.
	bulk_transfer :: proc(dev_handle: Device_Handle, endpoint: u8, data: [^]u8, length: c.int, transferred: ^c.int, timeout: c.uint) -> Error ---
	// Perform a USB interrupt transfer. Behaves like `bulk_transfer()` but for
	// interrupt endpoints. Returns SUCCESS or an Error.
	interrupt_transfer :: proc(dev_handle: Device_Handle, endpoint: u8, data: [^]u8, length: c.int, transferred: ^c.int, timeout: c.uint) -> Error ---
}

// ---------------------------------------------------------------------------------------------------------------------
// ----- Helper Procedures (from libusb static inline in libusb.h) ------------------------
// ---------------------------------------------------------------------------------------------------------------------

// Convert a 16-bit value from host-endian to little-endian format.
cpu_to_le16 :: #force_inline proc "contextless" (x: u16) -> u16 {
	return transmute(u16)u16le(x)
}

// Convert a 16-bit value from little-endian to host-endian format.
// Identical to `cpu_to_le16` since the conversion is its own inverse.
le16_to_cpu :: cpu_to_le16

// Get the data section of a control transfer. The data starts 8 bytes into
// the buffer, after the setup packet.
control_transfer_get_data :: #force_inline proc "contextless" (transfer: ^Transfer) -> [^]u8 {
	return ([^]u8)(&transfer.buffer[CONTROL_SETUP_SIZE])
}

// Get the control setup packet from the start of a transfer's data buffer.
control_transfer_get_setup :: #force_inline proc "contextless" (transfer: ^Transfer) -> ^Control_Setup {
	return (^Control_Setup)(transfer.buffer)
}

// Populate the setup packet (first 8 bytes of the data buffer) for a control
// transfer. The wValue, wIndex, and wLength values should be given in
// host-endian byte order; they will be converted to little-endian.
fill_control_setup :: proc "contextless" (
	buffer: [^]u8,
	bmRequestType: u8,
	bRequest: u8,
	wValue: u16,
	wIndex: u16,
	wLength: u16,
) {
	setup := (^Control_Setup)(buffer)
	setup.bmRequestType = bmRequestType
	setup.bRequest = bRequest
	setup.wValue = cpu_to_le16(wValue)
	setup.wIndex = cpu_to_le16(wIndex)
	setup.wLength = cpu_to_le16(wLength)
}

// Populate the required fields for a control transfer. If buffer is non-nil,
// the first 8 bytes are interpreted as a setup packet and the transfer length
// is inferred from the setup's wLength field.
fill_control_transfer :: proc "contextless" (
	transfer: ^Transfer,
	dev_handle: Device_Handle,
	buffer: [^]u8,
	callback: Transfer_Cb,
	user_data: rawptr,
	timeout: c.uint,
) {
	transfer.dev_handle = dev_handle
	transfer.endpoint = 0
	transfer.type = .CONTROL
	transfer.timeout = timeout
	transfer.buffer = buffer
	if buffer != nil {
		setup := (^Control_Setup)(buffer)
		transfer.length = c.int(CONTROL_SETUP_SIZE) + c.int(le16_to_cpu(setup.wLength))
	}
	transfer.user_data = user_data
	transfer.callback = callback
}

// Populate the required fields for a bulk transfer.
fill_bulk_transfer :: proc "contextless" (
	transfer: ^Transfer,
	dev_handle: Device_Handle,
	endpoint: u8,
	buffer: [^]u8,
	length: c.int,
	callback: Transfer_Cb,
	user_data: rawptr,
	timeout: c.uint,
) {
	transfer.dev_handle = dev_handle
	transfer.endpoint = endpoint
	transfer.type = .BULK
	transfer.timeout = timeout
	transfer.buffer = buffer
	transfer.length = length
	transfer.user_data = user_data
	transfer.callback = callback
}

// Populate the required fields for a bulk stream transfer.
// Since version 1.0.19.
fill_bulk_stream_transfer :: proc "contextless" (
	transfer: ^Transfer,
	dev_handle: Device_Handle,
	endpoint: u8,
	stream_id: u32,
	buffer: [^]u8,
	length: c.int,
	callback: Transfer_Cb,
	user_data: rawptr,
	timeout: c.uint,
) {
	fill_bulk_transfer(transfer, dev_handle, endpoint, buffer, length, callback, user_data, timeout)
	transfer.type = .BULK_STREAM
	transfer_set_stream_id(transfer, stream_id)
}

// Populate the required fields for an interrupt transfer.
fill_interrupt_transfer :: proc "contextless" (
	transfer: ^Transfer,
	dev_handle: Device_Handle,
	endpoint: u8,
	buffer: [^]u8,
	length: c.int,
	callback: Transfer_Cb,
	user_data: rawptr,
	timeout: c.uint,
) {
	transfer.dev_handle = dev_handle
	transfer.endpoint = endpoint
	transfer.type = .INTERRUPT
	transfer.timeout = timeout
	transfer.buffer = buffer
	transfer.length = length
	transfer.user_data = user_data
	transfer.callback = callback
}

// Populate the required fields for an isochronous transfer.
fill_iso_transfer :: proc "contextless" (
	transfer: ^Transfer,
	dev_handle: Device_Handle,
	endpoint: u8,
	buffer: [^]u8,
	length: c.int,
	num_iso_packets: c.int,
	callback: Transfer_Cb,
	user_data: rawptr,
	timeout: c.uint,
) {
	transfer.dev_handle = dev_handle
	transfer.endpoint = endpoint
	transfer.type = .ISOCHRONOUS
	transfer.timeout = timeout
	transfer.buffer = buffer
	transfer.length = length
	transfer.num_iso_packets = num_iso_packets
	transfer.user_data = user_data
	transfer.callback = callback
}

// Set the length of all packets in an isochronous transfer to the same value.
set_iso_packet_lengths :: proc "contextless" (transfer: ^Transfer, length: c.uint) {
	descs := ([^]Iso_Packet_Descriptor)(&transfer.iso_packet_desc)
	for i in 0 ..< int(transfer.num_iso_packets) {
		descs[i].length = length
	}
}

// Locate the position of an isochronous packet within the buffer by
// accumulating lengths of all preceding packets.
get_iso_packet_buffer :: proc "contextless" (transfer: ^Transfer, packet: c.uint) -> [^]u8 {
	if c.int(packet) >= transfer.num_iso_packets do return nil
	descs := ([^]Iso_Packet_Descriptor)(&transfer.iso_packet_desc)
	offset: uint = 0
	for i in 0 ..< int(packet) {
		offset += uint(descs[i].length)
	}
	return ([^]u8)(&transfer.buffer[offset])
}

// Locate the position of an isochronous packet within the buffer, assuming
// all packets are the same size as the first packet.
get_iso_packet_buffer_simple :: proc "contextless" (transfer: ^Transfer, packet: c.uint) -> [^]u8 {
	if c.int(packet) >= transfer.num_iso_packets do return nil
	descs := ([^]Iso_Packet_Descriptor)(&transfer.iso_packet_desc)
	offset := uint(descs[0].length) * uint(packet)
	return ([^]u8)(&transfer.buffer[offset])
}

// Retrieve a descriptor from the default control pipe. Convenience wrapper
// around `control_transfer()`.
get_descriptor :: proc(
	dev_handle: Device_Handle,
	desc_type: u8,
	desc_index: u8,
	data: [^]u8,
	length: c.int,
) -> c.int {
	return control_transfer(
		dev_handle,
		u8(Endpoint_Direction.IN),
		u8(Standard_Request.GET_DESCRIPTOR),
		u16(desc_type) << 8 | u16(desc_index),
		0,
		data,
		u16(length),
		1000,
	)
}

// Retrieve a string descriptor from a device. The string returned is Unicode
// (UTF-16LE) as per the USB spec. Convenience wrapper around `control_transfer()`.
get_string_descriptor :: proc(
	dev_handle: Device_Handle,
	desc_index: u8,
	langid: u16,
	data: [^]u8,
	length: c.int,
) -> c.int {
	return control_transfer(
		dev_handle,
		u8(Endpoint_Direction.IN),
		u8(Standard_Request.GET_DESCRIPTOR),
		u16(u16(Descriptor_Type.STRING) << 8 | u16(desc_index)),
		langid,
		data,
		u16(length),
		1000,
	)
}

// =============================================================================
// Tests
// =============================================================================

import "core:testing"

@(test)
init_test :: proc(t: ^testing.T) {
	result := init(nil)
	testing.expect_value(t, result, Error.SUCCESS)
	if result == .SUCCESS {
		exit(nil)
	}
}
